**Motion Capture Protocol:**

1. Open up Motive (current version 1.6 beta), make sure all the cameras are online. If not, reconnect the USB cables on the undetected cameras.
2. Calibrate the position of the cameras by wanding or simply load the previous calibration file.